	
	
	



Specifiers: Click on the ¶ icon in the WORD toolbar to reveal detailed instructions
(Specifier Note:  The purpose of this guide specification is to assist the specifier in correctly specifying wall panel products and execution.  The specifier needs to edit the guide specifications to fit the needs of specific projects.  Contact a Kingspan Insulated Panels Product Representative to assist in appropriate product selections.  Throughout the guide specification, there are Specifier Notes to assist in the editing of the file.

References have been made within the text of the specification to MasterFormat 2004 Section numbers and titles, specifier need to coordinate this numbers and titles with sections included for the specific project.  Brackets [ ]; “MAINTAIN”, “COORDINATE”, “EDIT”; and “DELETE” have been used to indicate when a selection is required.

This guide is for insulated exterior metal wall panels or interior metal wall panel partitions composed of a core of mineral fiber insulation attached with adhesive to and interior and exterior metal facings. This panel is designed to reduce the time required for installation by providing a single component assembly that provides the exterior weather barrier, high efficiency insulating core and an integral vapor barrier all-in-one. This panel offers energy cost savings through high R values and superior air and weathertightness.  
SECTION 07 42 13 
METAL CEILING PANELS
Kingspan Insulated Panels
Kingspan K-Roc HF Series Insulated Ceiling Panel System
GENERAL
SECTION INCLUDES
Steel faced, mineral wool core fire resistive insulated ceiling panels for [interior partitions] [interior fire rated partitions] [and] [ceilings]
Accessories including fasteners and perimeter trim
REFERENCES
ASTM International
ASTM A653: Standard Specification for Steel Sheet, Zinc-Coated (Galvanized) or Zinc-Iron Alloy-Coated (Galvannealed) by the Hot-Dip Process
ASTM A755: Standard Specification for Steel Sheet, Metallic Coated by the Hot-Dip Process and Prepainted by the Coil-Coating Process for Exterior Exposed Building Products
ASTM A792: Standard Specification for Steel Sheet, 55% Aluminum-Zinc Alloy-Coated by the Hot-Dip Process
ASTM A924: Standard Specification for General Requirements for Steel Sheet, Metallic-Coated by the Hot-Dip Process
ASTM C165: Standard Test Method for Measuring Compressive Properties of Thermal Insulations
ASTM C303: Standard Test Method for Dimensions and Density of Preformed Block and Board-Type Thermal Insulation
ASTM C518: Standard Test Method for Steady-State Thermal Transmission Properties by Means of the Heat Flow Meter Apparatus
ASTM C612: Standard Specification for Mineral Fiber Block and Board Thermal Insulation 
ASTM E72: Standard Test Methods of Conducting Strength Tests of Panels for Building Construction
ASTM E84: Standard Test Method for Surface Burning Characteristics of Building Materials
ASTM E119: Standard Test Methods for Fire Tests of Building Construction and Materials  
ASTM E136: Standard Test Method for Behavior of Materials in a Vertical Tube Furnace at 750° C
ASTM C1104: Standard Test Method for Determining the Water Vapor Sorption of Unfaced Mineral Fiber Insulation
ASTM C356: Standard Test Method for Linear Shrinkage of Preformed High-Temperature Thermal Insulation Subjected to Soaking Heat
ASTM E814: Standard Test Method for Fire Tests of Penetration Firestop Systems
Underwriters Laboratories (UL)

UL Canada (ULC)Approval:  
CAN/ULC-S101: Standard Methods of Fire Endurance Tests of Building Construction and Materials
CAN/ULC-S114: Standard Method of Test for Determination of Non-Combustibility in Building Materials
CAN/ULC-S115: Standard Method of Fire Tests of Firestop Systems
CAN/ULC-S102: Standard Method of Test for Surface Burning Characteristics of Building Materials and Assemblies
FM Global (FM)

Approval Standard 4880; Class 1 Fire Rating of Insulated Wall or Wall and Roof/Ceiling Panels, Interior Finish Materials or Coatings, and Exterior Wall Systems.

SUBMITTALS
(Specifier Note: DELETE Submittal Procedures paragraph when not required. Coordinate requirements with Division 01, Section 01 33 00 – Submittal Procedures.)

Refer to Section [01 33 00 Submittal Procedures] [insert section number and title]. 
Product Data:  Submit manufacturer current technical literature for each type of product.
Shop Drawings - Submit detailed drawings showing:
Profile 
Gauge of both exterior and interior sheet 
Location, layout and dimensions of panels
Location and type of fasteners
Shape and method of attachment of all trim
Locations and type of sealants 
Installation sequence
Coordination Drawings: Provide elevation drawings and building sections which show panels in relationship to required locations for structural support.  Include panel details and details showing attachment to structural support.
Other details as may be required for a weathertight installation
Panel Analysis: Provide panel calculations to indicate compliance with maximum deflection of [L/240] for the indicated ceiling design loads. The design load / deflection criteria and fastening pattern shall be verified from witnessed / audited tests using the “Chamber Method” in accordance with ASTM E72. Include effects of thermal differential between the exterior and interior panel facings.
Samples: Provide nominal 3 x 5 inch of each color indicated.  [Provide panel width by 10 inches long minimum] [Insert size].
(Specifier Note:  DELETE LEED submittal requirements when project is not pursuing LEED certification.  Related to Innovation and Design process (ID) credits; contact Kingspan for assistance in developing credits where their products can assist in obtaining. LEED-NC v2.2 credits are in red LEED-NC v3 credits are in red bold.)
LEED Submittals: 
(Specifier Note: Kingspan can provide whole building energy analysis reports, indicating how the use of Kingspan panels can assist in optimizing energy performance)
Energy and Atmosphere 
Energy Analysis: Demonstrating percentage of performance improvement compared with the baseline building performance rating. 
Material and Resources 
Building Life-Cycle Impact Reduction
Indoor Environmental Quality 
Low Emitting Materials: Compliance sheets indicating adhesives and gasket are within the published VOC emissions thresholds
Innovation in Design (ID)
Documentation for Credit: [Include specific requirements related to documenting credit.]
Quality Assurance Submittals
(Specifier Note:  DELETE Design Data, Test Report submittal requirements when propriety specification is used.  MAINTAIN Design Data, Test Report submittal requirement when other products may be submitted as substitutions.)
Design Data, Test Reports: Provide manufacturer test reports indicating product compliance with requirements.
Manufacturer Erection Instructions: Provide manufacturer’s written installation instructions including proper material storage, material handling, installation sequence, panel location(s), and attachment methods, details and required trim and accessories. 
QUALITY ASSURANCE
Manufacturer Qualifications: Manufacturer shall have a minimum of five (5) years experience in the production of fire resistive insulated metal panels.  Manufacturer shall demonstrate past experience with examples of projects of similar type and exposure.
Installer Qualifications:
Installer shall be authorized by the manufacturer and the work shall be supervised by a person having successfully completed a manufacturer training seminar regarding proper installation of the specified product.  
DELIVERY, STORAGE, AND HANDLING
(Specifier Note: DELETE Product Requirement paragraph when not required. Coordinate requirements with Division 01, Section 01 60 00 – Product Requirements.)
Refer to Section [01 60 00 Product Requirements] [insert section number and title].
Deliver panel materials and components in manufacturer’s original, unopened, undamaged packaging with identification labels intact.
Store ceiling panel materials on dry, level, firm, and clean surface.  Stack no more than two bundles high.  Elevate one end of bundle to allow moisture run-off, cover and ventilate to allow air to circulate and moisture to escape.  
Mineral fiber core shall be protected from moist air, rain and UV during construction. Stored panels must be wrapped in plastic or tarpaulins. Protect exposed mineral fiber from rain or water with plastic sheet during installation.
WARRANTY
Limited Panel Warranty: Standard form in which manufacturer agrees to repair or replace items that fail in materials or workmanship within specified warranty period. Coverage under the warranty includes panel performance, bond integrity, deflection and delamination. 
Warranty Period: Two (2) years from date of Substantial Completion, or 2 years and 6 months from the date of shipment from manufacturer’s plant, whichever occurs first.
(Specifier Note: Finish warranty periods are limited by the coil coater and the coating manufacturer and the finish.)

PRODUCTS
(Specifier Note: Product Information is proprietary to Kingspan Insulated Panels. If additional products are required for competitive procurement, contact Kingspan Insulated Panels for assistance.)
MANUFACTURER
Kingspan Insulated Panels Ltd. 12557 Coleraine Drive, Caledon, ON L7E 3B5 (866-442-3594); 5202-272nd Street, Langley, B.C. V4W 1S3 (866-442-3594) (www.kingspanpanels.ca); 
Kingspan Insulated Panels, Inc., 726 Summerhill Drive, Deland, FL 32724 (888-882-5862); 2000 Morgan Road, Modesto, CA 95358 (800-377-5110), 1509 Dewitt Ave, Mattoon, IL 61938 (www.kingspanpanels.us)  
Basis of Design: Kingspan K-Roc HF 
(Specifier Note: DELETE or COORDINATE Substitution Limitations paragraph if substitutions, are addressed in Division 01, Section 01 21 00 – Substitution Procedures.)
Substitution Limitations: 
Submit written request for approval of substitutions to the Architect [a minimum of [14] days prior to the date for receipt of bids] [Insert time period].  Include the following information:
Name of the materials and description of the proposed substitute.
Drawings, cut sheets, performance and test data.
List of projects similar scope and photographs of existing installations. 
Test reports indicating compliance with the performance criteria.
Other information necessary for evaluation.  
After evaluation by Architect, approval will be issued via addendum.  No verbal approval will be given. 
Substitutions following award of contract are not allowed except as stipulated in Division 01 – General Requirements.
[bookmark: _Hlk112916243]CEILING PANELS
Performance Criteria:
(Specifier Note:  Panel deflection of L/180 is manufacturer’s standard.  When other conditions dictate, deflection criteria may be different, insert appropriate criteria.)
Structural Test:  Structural performance shall be verifiable by witnessed structural testing for simulated wind loads in accordance with ASTM E72. Deflection criteria shall be [L/240] [insert project specific deflection criteria].
Thermal Properties: The panel mineral fiber core shall provide an R-value of 3.8 per inch thickness when tested in accordance with ASTM C518.    
Insulating Core:

Density:  8.5 lb. /cu. ft. +10%. -5%; in accordance with ASTM C303.
Combustibility: Does not meet the “pass” criteria, specified by ASTM E136.
Combustibility: Non-combustible when tested in accordance with ULC-S114.
Apparent thermal conductivity of mineral fiber core: R value / inch at 75º F. mean temp. - R=3.8 ft2 ºF h / Btu in in accordance with ASTM C518.
Compressive Strength: 45 kPa (6.5 psi) @ 10% compression in accordance with ASTM C165.
Dimensional stability: Linear shrinkage 0.2% at 1200º F in accordance with ASTM C356.
Moisture resistance: Water Vapor Sorption - 0.0 vol% in accordance with ASTM C1104.
Surface burning characteristics when tested in accordance with CAN/ULC S-102:
Flame Spread Rating: 0
Smoke Developed Classification: 0
Surface burning characteristics when tested in accordance with ASTM E84:
Flame Spread: 0
Smoke Developed: 0
Fire Test Response Characteristics: Steel-faced panels with mineral wool core shall comply with appropriate sections of Chapter 7 of the International Building Code regarding fire-resistance-rated construction.  The following approval listings/test reports shall be available upon request for submission to the Authority Having Jurisdiction:
ASTM E119: Panels shall have successfully passed the requirements of this standard when installed according to listed assembly.
CAN/ULC-S101: Panels shall have successfully passed the requirements of this standard when installed according to listed assembly.
CAN/ULC-S115: Panel penetrations shall have successfully passed the requirements of this standard when installed according to listed assembly.
ASTM E814: Panel penetrations shall have successfully passed the requirements of this standard when installed according to listed assembly.
Panel Description: 
(Specifier Note: Panel thickness is directly related to fire rating.  6 inch panels have 1 hour rating and 8 inch panel has 2 hour rating.)
Panel thickness: [6” – 60min], [6”- 90min], [8”- 2 hour]. thick.
Panel width: 42 inches.
Fire Rating: [6” – 60min], [6” – 90min], [8” - 2 hour].
Panel joint: Tongue and groove interlock joint. 
Reveal: 1/8 inch, 3/8 inch 
Exterior Face of Panel:
Material:
Steel coil material shall be in accordance with ASTM A755 ,Grade 33,[G90 galvanized steel in accordance with ASTM A653 and A924] [AZ50 Galvalume®/ Zincalume® (55% aluminum, 45% zinc) in accordance with ASTM A792],[Type 304 Stainless Steel].
(Specifier Note: Shadowline panel profile standard is 26 gauge with stucco embossed texture and is attached with exposed fasteners. Hidden fastened version requires minimum 24 gauge and is available in either stucco embossed or smooth texture). 
Profile: [Shadowline].
Profile description:  Linear striations nominal 0.0625 inch deep by ¾ inches wide at 3 inches on center.
Texture: [Non-directional stucco embossed] [Smooth]. 
Gauge:  [26] [24] [22]
4)       [24 gauge Type 304 Stainless Steel]
c.)OR
(Specifier Note: 24 gauge is standard for FLAT, MICRO-RIB, MINIMICRO-RIB and AZTECO panels). 
Profile: [Flat].
Profile description:  Flat (unprofiled)
Texture: [Non-directional stucco embossed] [Smooth].
Gauge:  [24] [22].
[Type 304 Stainless Steel 24ga – Flatness Waiver Required]
Profile: [Micro-Rib].
Profile description: Micro-Rib profile has linear 0.0625 inch deep fluted striations at ¾ inches on center. 
Texture: [Non-directional stucco embossed] [Smooth].
Gauge:  [24] [22].
OR
Profile: [Mini Micro-Rib].
Profile description: Mini Micro-Rib profile has linear 0.040 inch deep fluted striations at 5/16 inches on center. 
Texture: [Smooth].
Gauge:  [24] 
Profile: [Azteco].
Profile description: Azteco profile is flat.
Texture: Heavy (deeply) embossed.
Gauge:  [24] [22].

Color: [Selected from the current Kingspan Insulated Panels stock color chart] [Custom color as selected by Architect] [Color indicated].
(Specifier Note: Choose one of the following paint systems.  1.0 mil Two Coat system(Solid Color) is most commonly used.  Use the 2.4 mil Three Coat system if a harsh environment is anticipated (such as industrial facilities or in coastal regions). The 1.0 mil Mica color coat and the 1.5 mil Metallic color coat systems are chosen if Premium Colors are desired.  The paint systems will receive the 20 year finish warranty.
Interior Face of Panel:
Material:
Steel coil material shall be in accordance with ASTM A755 Grade 33,[G90 galvanized steel in accordance with ASTM A653 and A924] [AZ50 Galvalume®/ Zincalume® (55% aluminum, 45% zinc) in accordance with ASTM A792], [Type 304 Stainless Steel]. 
Profile: Shadowline.
Texture: [Non-directional stucco embossed] [Smooth].
 (Specifier Note: 26 gauge is standard). 
Gauge:  [26] [24], [Type 304 Stainless Steel 24ga]
Interior Finish: [modified polyester, dry film thickness of 1.0 mil including primer.] [PVDF finish, dry film thickness of 1.0 mil including primer] [Vinyl Plastisol, 4.0 mil including primer].
(Specifier Note: modified polyester “Imperial White” is standard finish and USDA accepted. PVDF “Regal White” is also USDA accepted. Vinyl Plastisol “White” is USDA accepted and is for use on interior surfaces only.  
Color: [USDA Imperial White] [Selected from the current Kingspan Insulated Panels stock color chart] [same as exterior finish] [Custom color as selected by Architect] [Color indicated].
Insulating Core: Rigid mineral wool insulation board, bonded with a thermal setting resin in accordance with ASTM C612.
ACCESSORIES
Fasteners:
[Exposed through-fasteners applied from the exterior side of the panel connecting both metal faces to supporting steel structure.]
OR
Material: Hex-head type with steel and neoprene washer
Material: Pancake-Head type fastener 
Size: As recommended by manufacturer. 
Perimeter Trim and Manding Plates:  
Required trim and metal flashing shall be steel with same coating, color, and gauge as the exterior face of the insulated metal ceiling panel, 

Plate Washer: 4”x4” 14ga Plate Washer
Mineral Wool: 8pcf  density Rockwool strips, Comfortboard 80, or Curtainrock 80 mineral wool
(Specifier Note: Sealants are a critical component for weatherization and fire rating.  Specific sealants are required for ASTM E119 fire rating.  See latest standard details for specific information
Sealants: 
1. Kingspan Butyl, non-skinning/curing, (per Kingspan K-Roc standard details) or type per panels manufacturer’s recommendations
2. Kingspan SAFIRE Intumescent Mastic Sealant (per Kingspan K-Roc standard details) or type per panels manufacturer’s recommendations
EXECUTION
EXAMINATION
Provide field measurements to manufacturer as required to achieve proper fit of the preformed ceiling panel.  Measurements shall be provided in a timely manner so that there is no impact to construction or manufacturing schedule.
Supporting Steel:  All structural supports required for installation of panels shall be by others.  
Examine individual panels upon removing from the bundle; notify manufacturer of panel defects.  Do not install defective panels.
Beginning of installation means acceptance of structure and supports for the installation of the insulated metal ceiling panels. 
PANEL INSTALLATION
Installation shall be in accordance with manufacturer’s installation guidelines and recommendations.
Install suspension system and panels true-to-line to dimensions and layout indicated on approved shop drawings.
Cut panels prior to installing, where indicated on shop drawings, using a power circular saw with fine tooth carbide tip blade per manufacturer’s instructions.    Personnel should wear respiratory and eye protection devices. 
Apply non-skinning butyl sealant and SAFIRE Intumescent Mastic as shown on shop drawings and manufacturer’s installation instructions so as to complete the necessary vapor barrier and fire rating.
(Specifier Note: Edit per project conditions, if no hidden clips delete paragraph.)
TRIM INSTALLATION  
Place trim and trim fasteners only as indicated per details on the approved shop drawings.
Place a continuous strip of butyl tape or butyl sealant on closure trims for the length of the panel to be covered as indicated on shop drawings.  
CLEANING AND PROTECTION
Remove protective film immediately after installation. 
Touch-up, repair or replace metal panels and trim that have been damaged.

END OF SECTION
DISCLAIMER: 

Kingspan Insulated Panels Guide Specifications have been written as an aid to the professionally qualified Specifier and Design Professional. The use of this Guideline Specification requires the sole professional judgment and expertise of the qualified Specifier and Design Professional to adapt the information to the specific needs for the Building Owner and the Project, to coordinate with their Construction Document Process, and to meet all the applicable building codes, regulations and laws. KINGSPAN INSULATED PANELS EXPRESSLY DISCLAIMS ANY WARRANTY, EXPRESSED OR IMPLIED, INCLUDING THE WARRANTY OF MERCHANTABILITY OR FITNESS FOR PARTICULAR PURPOSE OF THIS PRODUCT FOR THE PROJECT.
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